| Wireshark 4.7.0 The Wireshark network protocol analyzer

Loading...
Searching...
No Matches
Public Attributes | List of all members
mac_lte_info Struct Reference

## Public Attributes
uint8_t | radioType
uint8_t | direction
uint8_t | rntiType
uint16_t | rnti
uint16_t | ueid
uint16_t | sysframeNumber
uint16_t | subframeNumber
bool | sfnSfInfoPresent
bool | subframeNumberOfGrantPresent
uint16_t | subframeNumberOfGrant
bool | isPredefinedData
uint16_t | length
uint8_t | reTxCount
uint8_t | isPHICHNACK
bool | isExtendedBSRSizes
bool | isSimultPUCCHPUSCHPCell
bool | isSimultPUCCHPUSCHPSCell
bool | crcStatusValid
mac_lte_crc_status | crcStatus
mac_lte_carrier_id | carrierId
mac_lte_dl_retx | dl_retx
mac_lte_ce_mode | ceMode
mac_lte_nb_mode | nbMode
uint8_t | nUlRb
union { |
struct mac_lte_ul_phy_info { |
uint8_t present |
uint8_t modulation_type |
uint8_t tbs_index |
uint8_t resource_block_length |
uint8_t resource_block_start |
uint8_t harq_id |
bool ndi |
} ul_info |
struct mac_lte_dl_phy_info { |
uint8_t present |
uint8_t dci_format |
uint8_t resource_allocation_type |
uint8_t aggregation_level |
uint8_t mcs_index |
uint8_t redundancy_version_index |
uint8_t resource_block_length |
uint8_t harq_id |
bool ndi |
uint8_t transport_block |
} dl_info |
} | detailed_phy_info |
mac_lte_oob_event | oob_event
uint8_t | rapid
uint8_t | rach_attempt_number
uint16_t | number_of_srs
uint16_t | oob_ueid [MAX_SRs]
uint16_t | oob_rnti [MAX_SRs]

The documentation for this struct was generated from the following file:

- /builds/wireshark/wireshark/epan/dissectors/packet-mac-lte.h