| Wireshark 4.7.0 The Wireshark network protocol analyzer

Loading...
Searching...
No Matches
packet-s1ap.h
1/* Do not modify this file. Changes will be overwritten. */
2/* Generated automatically by the ASN.1 to Wireshark dissector compiler */
3/* packet-s1ap.h */
4/* asn2wrs.py -q -L -p s1ap -c ./s1ap.cnf -s ./packet-s1ap-template -D . -O ../.. S1AP-CommonDataTypes.asn S1AP-Constants.asn S1AP-Containers.asn S1AP-IEs.asn S1AP-PDU-Contents.asn S1AP-PDU-Descriptions.asn S1AP-SonTransfer-IEs.asn */
5
6/* packet-s1ap.h
7 * Routines for E-UTRAN S1 Application Protocol (S1AP) packet dissection
8 *
9 * Wireshark - Network traffic analyzer
10 * By Gerald Combs <gerald@wireshark.org>
11 * Copyright 1998 Gerald Combs
12 *
13 * SPDX-License-Identifier: GPL-2.0-or-later
14 */
15
16#ifndef PACKET_S1AP_H
17#define PACKET_S1AP_H
18
19 typedef struct _s1ap_ctx_t {
20 uint32_t message_type;
21 uint32_t ProcedureCode;
22 uint32_t ProtocolIE_ID;
23 uint32_t ProtocolExtensionID;
24} s1ap_ctx_t;
25
26extern const value_string s1ap_warningType_vals[];
27extern const value_string s1ap_serialNumber_gs_vals[];
28
29void dissect_s1ap_warningMessageContents(tvbuff_t *warning_msg_tvb, proto_tree *tree, packet_info *pinfo, uint8_t dcs, int hf_nb_pages, int hf_decoded_page);
30
31extern const value_string s1ap_Cause_vals[];
32extern const value_string s1ap_CauseMisc_vals[];
33extern const value_string s1ap_CauseProtocol_vals[];
34extern const value_string s1ap_CauseRadioNetwork_vals[];
35extern const value_string s1ap_CauseTransport_vals[];
36extern const value_string s1ap_CauseNas_vals[];
37extern const value_string s1ap_SONtransferRequestContainer_vals[];
38extern const value_string s1ap_SONtransferResponseContainer_vals[];
39int dissect_s1ap_Global_ENB_ID(tvbuff_t *tvb _U_, int offset _U_, asn1_ctx_t *actx _U_, proto_tree *tree _U_, int hf_index _U_);
40int dissect_s1ap_SONtransferRequestContainer(tvbuff_t *tvb _U_, int offset _U_, asn1_ctx_t *actx _U_, proto_tree *tree _U_, int hf_index _U_);
41int dissect_s1ap_SONtransferResponseContainer(tvbuff_t *tvb _U_, int offset _U_, asn1_ctx_t *actx _U_, proto_tree *tree _U_, int hf_index _U_);
42int dissect_s1ap_Global_ENB_ID_PDU(tvbuff_t *tvb _U_, packet_info *pinfo _U_, proto_tree *tree _U_, void *data _U_);
43int dissect_s1ap_ENB_StatusTransfer_TransparentContainer_PDU(tvbuff_t *tvb _U_, packet_info *pinfo _U_, proto_tree *tree _U_, void *data _U_);
44int dissect_s1ap_EN_DCSONConfigurationTransfer_PDU(tvbuff_t *tvb _U_, packet_info *pinfo _U_, proto_tree *tree _U_, void *data _U_);
45int dissect_s1ap_EUTRAN_CGI_PDU(tvbuff_t *tvb _U_, packet_info *pinfo _U_, proto_tree *tree _U_, void *data _U_);
46int dissect_s1ap_HandoverRestrictionList_PDU(tvbuff_t *tvb _U_, packet_info *pinfo _U_, proto_tree *tree _U_, void *data _U_);
47int dissect_s1ap_IntersystemSONConfigurationTransfer_PDU(tvbuff_t *tvb _U_, packet_info *pinfo _U_, proto_tree *tree _U_, void *data _U_);
48int dissect_s1ap_LastVisitedEUTRANCellInformation_PDU(tvbuff_t *tvb _U_, packet_info *pinfo _U_, proto_tree *tree _U_, void *data _U_);
49int dissect_s1ap_LastVisitedGERANCellInformation_PDU(tvbuff_t *tvb _U_, packet_info *pinfo _U_, proto_tree *tree _U_, void *data _U_);
50int dissect_s1ap_MDTMode_PDU(tvbuff_t *tvb _U_, packet_info *pinfo _U_, proto_tree *tree _U_, void *data _U_);
51int dissect_s1ap_PSCellInformation_PDU(tvbuff_t *tvb _U_, packet_info *pinfo _U_, proto_tree *tree _U_, void *data _U_);
52int dissect_s1ap_SONConfigurationTransfer_PDU(tvbuff_t *tvb _U_, packet_info *pinfo _U_, proto_tree *tree _U_, void *data _U_);
53int dissect_s1ap_SourceeNB_ToTargeteNB_TransparentContainer_PDU(tvbuff_t *tvb _U_, packet_info *pinfo _U_, proto_tree *tree _U_, void *data _U_);
54int dissect_s1ap_TargeteNB_ToSourceeNB_TransparentContainer_PDU(tvbuff_t *tvb _U_, packet_info *pinfo _U_, proto_tree *tree _U_, void *data _U_);
55int dissect_s1ap_UE_HistoryInformation_PDU(tvbuff_t *tvb _U_, packet_info *pinfo _U_, proto_tree *tree _U_, void *data _U_);
56int dissect_s1ap_SONtransferApplicationIdentity_PDU(tvbuff_t *tvb _U_, packet_info *pinfo _U_, proto_tree *tree _U_, void *data _U_);
57int dissect_s1ap_SONtransferRequestContainer_PDU(tvbuff_t *tvb _U_, packet_info *pinfo _U_, proto_tree *tree _U_, void *data _U_);
58int dissect_s1ap_SONtransferResponseContainer_PDU(tvbuff_t *tvb _U_, packet_info *pinfo _U_, proto_tree *tree _U_, void *data _U_);
59int dissect_s1ap_SONtransferCause_PDU(tvbuff_t *tvb _U_, packet_info *pinfo _U_, proto_tree *tree _U_, void *data _U_);
60
61#endif /* PACKET_S1AP_H */
62
63/*
64 * Editor modelines
65 *
66 * Local Variables:
67 * c-basic-offset: 2
68 * tab-width: 8
69 * indent-tabs-mode: nil
70 * End:
71 *
72 * ex: set shiftwidth=2 tabstop=8 expandtab:
73 * :indentSize=2:tabSize=8:noTabs=true:
74 */
_asn1_ctx_t
Definition asn1.h:66
_packet_info
Definition packet_info.h:43
_proto_node
Definition proto.h:907
_s1ap_ctx_t
Definition packet-s1ap.h:19
_value_string
Mapping between a 32-bit integer value and its string representation.
Definition value_string.h:33
tvbuff
Definition tvbuff-int.h:35