| Wireshark 4.7.0 The Wireshark network protocol analyzer

Loading...
Searching...
No Matches
packet-rrc.h
1/* Do not modify this file. Changes will be overwritten. */
2/* Generated automatically by the ASN.1 to Wireshark dissector compiler */
3/* packet-rrc.h */
4/* asn2wrs.py -q -L -p rrc -c ./rrc.cnf -s ./packet-rrc-template -D . -O ../.. Class-definitions.asn PDU-definitions.asn InformationElements.asn Constant-definitions.asn Internode-definitions.asn */
5
6/* packet-rrc-template.h
7 * Copyright 2009, Anders Broman <anders.broman@ericsson.com>
8 *
9 * Wireshark - Network traffic analyzer
10 * By Gerald Combs <gerald@wireshark.org>
11 * Copyright 1998 Gerald Combs
12 *
13 * SPDX-License-Identifier: GPL-2.0-or-later
14 */
15
16#ifndef PACKET_RRC_H
17#define PACKET_RRC_H
18
19#include <epan/asn1.h> /* Needed for non asn1 dissectors?*/
20
21extern int proto_rrc;
22int dissect_rrc_InterRATHandoverInfo(tvbuff_t *tvb _U_, int offset _U_, asn1_ctx_t *actx _U_, proto_tree *tree _U_, int hf_index _U_);
23int dissect_rrc_HandoverToUTRANCommand_PDU(tvbuff_t *tvb _U_, packet_info *pinfo _U_, proto_tree *tree _U_, void *data _U_);
24int dissect_rrc_InterRATHandoverInfo_PDU(tvbuff_t *tvb _U_, packet_info *pinfo _U_, proto_tree *tree _U_, void *data _U_);
25int dissect_rrc_MeasurementReport_PDU(tvbuff_t *tvb _U_, packet_info *pinfo _U_, proto_tree *tree _U_, void *data _U_);
26int dissect_rrc_MasterInformationBlock_PDU(tvbuff_t *tvb _U_, packet_info *pinfo _U_, proto_tree *tree _U_, void *data _U_);
27int dissect_rrc_SysInfoType1_PDU(tvbuff_t *tvb _U_, packet_info *pinfo _U_, proto_tree *tree _U_, void *data _U_);
28int dissect_rrc_SysInfoType2_PDU(tvbuff_t *tvb _U_, packet_info *pinfo _U_, proto_tree *tree _U_, void *data _U_);
29int dissect_rrc_SysInfoType3_PDU(tvbuff_t *tvb _U_, packet_info *pinfo _U_, proto_tree *tree _U_, void *data _U_);
30int dissect_rrc_SysInfoType4_PDU(tvbuff_t *tvb _U_, packet_info *pinfo _U_, proto_tree *tree _U_, void *data _U_);
31int dissect_rrc_SysInfoType5_PDU(tvbuff_t *tvb _U_, packet_info *pinfo _U_, proto_tree *tree _U_, void *data _U_);
32int dissect_rrc_SysInfoType6_PDU(tvbuff_t *tvb _U_, packet_info *pinfo _U_, proto_tree *tree _U_, void *data _U_);
33int dissect_rrc_SysInfoType7_PDU(tvbuff_t *tvb _U_, packet_info *pinfo _U_, proto_tree *tree _U_, void *data _U_);
34int dissect_rrc_SysInfoType11_PDU(tvbuff_t *tvb _U_, packet_info *pinfo _U_, proto_tree *tree _U_, void *data _U_);
35int dissect_rrc_SysInfoType12_PDU(tvbuff_t *tvb _U_, packet_info *pinfo _U_, proto_tree *tree _U_, void *data _U_);
36int dissect_rrc_SysInfoType13_PDU(tvbuff_t *tvb _U_, packet_info *pinfo _U_, proto_tree *tree _U_, void *data _U_);
37int dissect_rrc_SysInfoType13_1_PDU(tvbuff_t *tvb _U_, packet_info *pinfo _U_, proto_tree *tree _U_, void *data _U_);
38int dissect_rrc_SysInfoType13_2_PDU(tvbuff_t *tvb _U_, packet_info *pinfo _U_, proto_tree *tree _U_, void *data _U_);
39int dissect_rrc_SysInfoType13_3_PDU(tvbuff_t *tvb _U_, packet_info *pinfo _U_, proto_tree *tree _U_, void *data _U_);
40int dissect_rrc_SysInfoType13_4_PDU(tvbuff_t *tvb _U_, packet_info *pinfo _U_, proto_tree *tree _U_, void *data _U_);
41int dissect_rrc_SysInfoType14_PDU(tvbuff_t *tvb _U_, packet_info *pinfo _U_, proto_tree *tree _U_, void *data _U_);
42int dissect_rrc_SysInfoType15_PDU(tvbuff_t *tvb _U_, packet_info *pinfo _U_, proto_tree *tree _U_, void *data _U_);
43int dissect_rrc_SysInfoType15_1_PDU(tvbuff_t *tvb _U_, packet_info *pinfo _U_, proto_tree *tree _U_, void *data _U_);
44int dissect_rrc_SysInfoType15_2_PDU(tvbuff_t *tvb _U_, packet_info *pinfo _U_, proto_tree *tree _U_, void *data _U_);
45int dissect_rrc_SysInfoType15_3_PDU(tvbuff_t *tvb _U_, packet_info *pinfo _U_, proto_tree *tree _U_, void *data _U_);
46int dissect_rrc_SysInfoType15_4_PDU(tvbuff_t *tvb _U_, packet_info *pinfo _U_, proto_tree *tree _U_, void *data _U_);
47int dissect_rrc_SysInfoType16_PDU(tvbuff_t *tvb _U_, packet_info *pinfo _U_, proto_tree *tree _U_, void *data _U_);
48int dissect_rrc_SysInfoType17_PDU(tvbuff_t *tvb _U_, packet_info *pinfo _U_, proto_tree *tree _U_, void *data _U_);
49int dissect_rrc_SysInfoType18_PDU(tvbuff_t *tvb _U_, packet_info *pinfo _U_, proto_tree *tree _U_, void *data _U_);
50int dissect_rrc_SysInfoType19_PDU(tvbuff_t *tvb _U_, packet_info *pinfo _U_, proto_tree *tree _U_, void *data _U_);
51int dissect_rrc_SysInfoTypeSB1_PDU(tvbuff_t *tvb _U_, packet_info *pinfo _U_, proto_tree *tree _U_, void *data _U_);
52int dissect_rrc_SysInfoTypeSB2_PDU(tvbuff_t *tvb _U_, packet_info *pinfo _U_, proto_tree *tree _U_, void *data _U_);
53int dissect_rrc_ToTargetRNC_Container_PDU(tvbuff_t *tvb _U_, packet_info *pinfo _U_, proto_tree *tree _U_, void *data _U_);
54int dissect_rrc_TargetRNC_ToSourceRNC_Container_PDU(tvbuff_t *tvb _U_, packet_info *pinfo _U_, proto_tree *tree _U_, void *data _U_);
55
56enum rrc_message_type {
57 RRC_MESSAGE_TYPE_INVALID = 0,
58 RRC_MESSAGE_TYPE_PCCH = 1,
59 RRC_MESSAGE_TYPE_UL_CCCH,
60 RRC_MESSAGE_TYPE_DL_CCCH,
61 RRC_MESSAGE_TYPE_UL_DCCH,
62 RRC_MESSAGE_TYPE_DL_DCCH,
63 RRC_MESSAGE_TYPE_BCCH_FACH
64};
65
66enum nas_sys_info_gsm_map {
67 RRC_NAS_SYS_UNKNOWN = 0,
68 RRC_NAS_SYS_INFO_CS,
69 RRC_NAS_SYS_INFO_PS,
70 RRC_NAS_SYS_INFO_CN_COMMON
71};
72
73enum rrc_ue_state {
74 RRC_UE_STATE_UNKNOWN = 0,
75 RRC_UE_STATE_CELL_DCH,
76 RRC_UE_STATE_CELL_FACH,
77 RRC_UE_STATE_CELL_PCH,
78 RRC_UE_STATE_URA_PCH
79};
80
81#define MAX_RRC_FRAMES 64
82 typedef struct rrc_info
83{
84 enum rrc_message_type msgtype[MAX_RRC_FRAMES];
85 uint16_t hrnti[MAX_RRC_FRAMES];
86} rrc_info;
87
88/*Struct for storing ciphering information*/
89 typedef struct rrc_ciphering_info
90{
91 int seq_no[31][2]; /*Indicates for each Rbid when ciphering starts - Indexers are [BearerID][Direction]*/
92 GTree * /*uint32_t*/ start_cs; /*Start value for CS counter*/
93 GTree * /*uint32_t*/ start_ps; /*Start value for PS counter*/
94 int32_t ciphering_algorithm; /*Indicates which type of ciphering algorithm used*/
95 int32_t integrity_algorithm; /*Indicates which type of integrity algorithm used*/
96 uint32_t setup_frame[2]; /*Store which frame contained this information - Indexer is [Direction]*/
97 uint32_t ps_conf_counters[31][2]; /*This should also be made for CS*/
98
99} rrc_ciphering_info;
100
101extern GTree * hsdsch_muxed_flows;
102extern GTree * rrc_ciph_info_tree;
103extern wmem_tree_t* rrc_global_urnti_crnti_map;
104
105#endif /* PACKET_RRC_H */
asn1.h
_asn1_ctx_t
Definition asn1.h:66
_packet_info
Definition packet_info.h:43
_proto_node
Definition proto.h:907
_wmem_tree_t
Internal representation of a wmem balanced tree.
Definition wmem_tree-int.h:81
rrc_ciphering_info
Definition packet-rrc.h:90
rrc_info
Definition packet-rrc.h:83
tvbuff
Definition tvbuff-int.h:35