| Wireshark 4.7.0 The Wireshark network protocol analyzer

Loading...
Searching...
No Matches
packet-csn1.h
1/* packet-csn1.h
2 * Declarations and types for CSN1 dissection in wireshark.
3 * By Vincent Helfre, based on original code by Jari Sassi
4 * with the gracious authorization of STE
5 * Copyright (c) 2011 ST-Ericsson
6 *
7 * Wireshark - Network traffic analyzer
8 * By Gerald Combs <gerald@wireshark.org>
9 * Copyright 1998 Gerald Combs
10 *
11 * SPDX-License-Identifier: GPL-2.0-or-later
12 */
13
14#ifndef _PACKET_CSN1_H_
15#define _PACKET_CSN1_H_
16
17#include <epan/expert.h>
18#include <wsutil/array.h>
19
20/* Error codes */
21#define CSN_OK 0
22#define CSN_ERROR_GENERAL -1
23#define CSN_ERROR_DATA_NOT_VALID -2
24#define CSN_ERROR_IN_SCRIPT -3
25#define CSN_ERROR_INVALID_UNION_INDEX -4
26#define CSN_ERROR_NEED_MORE_BITS_TO_UNPACK -5
27#define CSN_ERROR_ILLEGAL_BIT_VALUE -6
28#define CSN_ERROR_INTERNAL -7
29#define CSN_ERROR_STREAM_NOT_SUPPORTED -8
30#define CSN_ERROR_MESSAGE_TOO_LONG -9
31#define CSN_ERROR_ -10
32
33/* CallBack return status */
34typedef int16_t CSN_CallBackStatus_t;
35
36#define CSNCBS_OK 0
37#define CSNCBS_NOT_OK -10
38#define CSNCBS_NOT_TO_US -11
39#define CSNCBS_NOT_COMPLETE -12
40
41#define CSNCBS_REVISION_LIMIT_STOP -20 /* Stop packing/unpacking - revision limit */
42#define CSNCBS_NOT_SUPPORTED_IE -21 /* Handling of the unpacked IE is not supported by MS-software */
43
44typedef void(*void_fn_t)(void);
45
46/* Context holding CSN1 parameters */
47 typedef struct
48{
49 int remaining_bits_len; /* IN to an csn stream operation */
50 int bit_offset; /* IN/OUT to an csn stream operation */
51 packet_info* pinfo;
52} csnStream_t;
53
54typedef int16_t (*StreamSerializeFcn_t)(proto_tree *tree, csnStream_t* ar, tvbuff_t *tvb, void* data, int ett_csn1);
55typedef CSN_CallBackStatus_t (*DissectorCallbackFcn_t)(proto_tree *tree, tvbuff_t *tvb, void* param1, void* param2, int bit_offset, int ett_csn1, packet_info* pinfo);
56
57
58typedef enum
59{
60 CSN_END = 0,
61 CSN_BIT,
62 CSN_UINT,
63 CSN_TYPE,
64 CSN_CHOICE,
65 CSN_UNION,
66 CSN_UNION_LH,
67 CSN_UINT_ARRAY,
68 CSN_TYPE_ARRAY,
69 CSN_BITMAP, /* Bitmap with constant: <bitmap: bit(64)> */
70 CSN_VARIABLE_BITMAP, /* <N: bit (5)> <bitmap: bit(N + offset)> */
71 CSN_VARIABLE_BITMAP_1, /* <bitmap: bit**> i.e. to the end of message (R99) */
72 CSN_LEFT_ALIGNED_VAR_BMP, /* As variable bitmap but the result is left aligned (R99) */
73 CSN_LEFT_ALIGNED_VAR_BMP_1,/* As above only size is to the end of message (R99) */
74 CSN_PADDING_BITS, /* Padding bits fill to the end of the buffer */
75 CSN_VARIABLE_ARRAY, /* Array with length specified in parameter: <N: bit(4)> <list: octet(N + offset)> */
76 CSN_VARIABLE_TARRAY, /* Type Array with length specified in parameter: <N: bit(x)> <Type>*N */
77 CSN_VARIABLE_TARRAY_OFFSET,/* As above but with offset. The offset is stored as third parameter of CSN_DESCR (descr.value) */
78 CSN_RECURSIVE_ARRAY, /* Recursive way to specify an array of uint: <list> ::= {1 <number: bit(4) <list>|0}; */
79 CSN_RECURSIVE_TARRAY, /* Recursive way to specify an array of type: <list> ::= {1 <type>} ** 0 ; */
80 CSN_RECURSIVE_TARRAY_1, /* same as above but first element always exist:<list> ::= <type> {1 <type>} ** 0 ; */
81 CSN_RECURSIVE_TARRAY_2, /* same as above but with reversed separators :<lists> ::= <type> { 0 <type> } ** 1 ; */
82 CSN_EXIST,
83 CSN_EXIST_LH,
84 CSN_NEXT_EXIST,
85 CSN_NEXT_EXIST_LH,
86 CSN_NULL,
87 CSN_FIXED,
88 CSN_CALLBACK,
89 CSN_UINT_OFFSET, /* unpack will add offset, inverse pack will subtract offset */
90 CSN_UINT_LH, /* Low High extraction of int */
91 CSN_SERIALIZE,
92 CSN_SPLIT_BITS,
93 CSN_SPLIT_BITS_CRUMB,
94 CSN_TRAP_ERROR
95} csn_type_t;
96
97/******************************************************************************************
98 * CSN_DESCR structure:
99 *
100 * type:
101 * This is the CSN type. All existing types are specified in the section above.
102 *
103 * i:
104 * Depending on the contents of the type parameter, the parameter "i" may have following meaning:
105 * - specifies the number of bits for the CSN_UINT or CSN_UINT_OR_NULL types
106 * - the offset for an array size by which the size is incremented
107 * for the CSN_VAR_ARRAY type
108 * - the length of each element of an array for the CSN_REC_ARRAY type
109 * - the number of the elements in an array for the CSN_TYPE_ARRAY type
110 * - the offset to the variable keeping the number of elements of an array for in the CSN_VAR_TARRAY type
111 * - the number of different data types in a union for the CSN_UNION, CSN_UNION_LH, and for the CSN_CHOICE types
112 * - the length in bits of the fixed number defined for the CSN_FIXED type
113 * - the number of lines to skip in the CSN_DESCR type specified for the CSN_NEXT_EXIST, CSN_NEXT_EXIST_LH,
114 * CSN_NEXT_EXIST_OR_NULL, and CSN_NEXT_EXIST_OR_NULL_LH types
115 * - the number of bits in a bitmap for the CSN_BITMAP type
116 * - the value by which the number of bits in a bitmap has to be incremented or decremented for the
117 * CSN_VAR_BITMAP, CSN_LEFT_VAR_BMP, and CSN_LEFT_BMP_1 types
118 * - the offset to param1 for the CSN_CALLBACK type
119 * - ERRORCODE used by the CSN_ERROR type
120 * - the bit-length of the LENGTH field in a CSN_SERIALISE type
121 *
122 * descr
123 * This parameter has different meaning depending on the value of the type parameter:
124 * - the offset for the CSN_UINT_OFFSET type
125 * - the number of the elements in an array of the CSN_UINT_ARRAY type
126 * - the offset to the parameter where the size of the array has to be stored for the CSN_REC_ARRAY type
127 * - the address of the internal structure, describing the member type (by means of the CSN_DESCR type) in the
128 * CSN_TYPE_ARRAY, CSN_VAR_TARRAY, and CSN_TYPE types
129 * - the address of the variable of type CSN_ChoiceElement_t describing all elements in the CSN_CHOICE type union
130 * - the offset to the variable where the number of bits has to be or is stored for the CSN_VAR_BITMAP,
131 * CSN_LEFT_VAR_BMP, and CSN_LEFT_BMP_1 types
132 * - the function number (case number) for the CSN_CALLBACK and CSN_CALLBACK_NO_ARGS types
133 * - the free text used by the CSN_TRAP_ERROR
134 *
135 * offset
136 * This is an offset to the _MEMBER parameter counting from the beginning of struct
137 * where the unpacked or packed value shall be stored or fetched. The meaning of the _MEMBER parameter
138 * varies depending on the type which is specified and so is the meaning of the offset parameter.
139 * Some types (and corresponding macros) do not have the _MEMBER parameter and then the offset parameter
140 * is not used or is different from the offset to the _MEMBER.
141 * - the fixed value for the CSN_FIXED type
142 * - an offset to the variable UnionType for CSN_UNION and CSN_UNION_LH types
143 * - an offset to the variable Exist for CSN_NEXT_EXIST and CSN_NEXT_EXIST_LH types
144 * - an offset to param2 in the CSN_CALLBACK type
145 *
146 * may_be_null
147 * true: if dissection may be attempted at an offset beyond the length of existing data bits
148 * false: othewise
149 *
150 * sz
151 * - is the name of the parameter within the descr where their unpacked or packed value shall be stored or fetched.
152 * This parameter is pointed out by the offset parameter in the same CSN_DESCR variable as the sz.
153 * - the free text used by the CSN_TRAP_ERROR (the same as parameter "i")
154 *
155 * serialize
156 * - stores the size of _MEMBER type in case of the M_TYPE_ARRAY and M_VAR_TARRAY,
157 * - the address of the function which is provided by the M_SERIALIZE type.
158 ******************************************************************************************/
159
160
161 typedef struct
162{
163 int16_t type;
164 int16_t i;
165 union
166 {
167 const void* ptr;
168 uint32_t value;
169 const crumb_spec_t *crumb_spec;
170 } descr;
171 size_t offset;
172 bool may_be_null;
173 const char* sz;
174 expert_field* error;
175 uint32_t value;
176 int* hf_ptr;
177 /* used in M_REC_ARRAY to distinguish between "field" and "field exists",
178 it's not used on fields that just "exist" */
179 int* hf_exist_ptr;
180 void_fn_t aux_fn;
181} CSN_DESCR;
182
183 typedef struct
184{
185 uint8_t bits;
186 uint8_t value;
187 bool keep_bits;
188 CSN_DESCR descr;
189} CSN_ChoiceElement_t;
190
191void csnStreamInit(csnStream_t* ar, int BitOffset, int BitCount, packet_info* pinfo);
192
193/******************************************************************************
194* FUNCTION: csnStreamDissector
195* DESCRIPTION:
196* UnPacks data from bit stream. According to CSN description.
197* ARGS:
198* ar stream will hold the parameters to the pack function
199* ar->remaining_bits_len [IN] Number of bits to unpack [OUT] number of bits left to unpack.
200* ar->bit_offset [IN/OUT] is the current bit where to proceed with the next bit to unpack.
201
202* pDescr CSN description.
203* tvb buffer containing the bit stream to unpack.
204* data unpacked data.
205* ett_csn1 tree
206*
207* RETURNS: int Number of bits left to be unpacked. Negative Error code if failed to unpack all bits
208******************************************************************************/
209int16_t csnStreamDissector(proto_tree *tree, csnStream_t* ar, const CSN_DESCR* pDescr, tvbuff_t *tvb, void* data, int ett_csn1);
210
211/* CSN struct macros */
212#define CSN_DESCR_BEGIN(_STRUCT)\
213 CSN_DESCR CSNDESCR_##_STRUCT[] = {
214
215#define CSN_DESCR_END(_STRUCT)\
216 {CSN_END, 0, {0}, 0, false, "", NULL, 0, NULL, NULL, NULL} };
217
218/******************************************************************************
219 * CSN_ERROR(Par1, Par2, Par3)
220 * May be called at any time when an abort of packing or unpacking of a message
221 * is desired
222 * Par1: C structure name
223 * Par2: free text which will appear in the error handler
224 * Par3: Error code
225 *****************************************************************************/
226#define CSN_ERROR(_STRUCT, _Text, _ERRCODE, _EI_ERROR)\
227 {CSN_TRAP_ERROR, _ERRCODE, {_Text}, 0, false, _Text, _EI_ERROR, 0, NULL, NULL, NULL}
228
229/******************************************************************************
230 * M_BIT(Par1, Par2, Par3)
231 * Defines one bit element in the CSN1 syntax.
232 * Par1: C structure name
233 * Par2: C structure element name
234 * Par3: pointer to the header field
235 *****************************************************************************/
236#define M_BIT(_STRUCT, _MEMBER, _HF_PTR)\
237 {CSN_BIT, 0, {0}, offsetof(_STRUCT, _MEMBER), false, #_MEMBER, NULL, 0, _HF_PTR, NULL, NULL}
238
239/******************************************************************************
240 * M_BIT_OR_NULL(Par1, Par2, Par3)
241 * Similar to the M_BIT except that not only bit 0 or 1 but also the
242 * end of the message may be encountered when looking for the next element in
243 * the message.
244 * Covers the case {null | 0 | 1}
245 *****************************************************************************/
246#define M_BIT_OR_NULL(_STRUCT, _MEMBER, _HF_PTR)\
247 {CSN_BIT, 0, {0}, offsetof(_STRUCT, _MEMBER), true, #_MEMBER, NULL, 0, _HF_PTR, NULL, NULL}
248/******************************************************************************
249 * M_NEXT_EXIST(Par1, Par2, Par3)
250 * Indicates whether the next element or a group of elements defined in the
251 * structure is present or not.
252 * Par1: C structure name
253 * Par2: C structure element name
254 * Par3: number of lines to skip in the CSN_DESCR type specified if the
255 * element(s) does not exist
256 *****************************************************************************/
257#define M_NEXT_EXIST(_STRUCT, _MEMBER, _NoOfExisting, _HF_PTR)\
258 {CSN_NEXT_EXIST, _NoOfExisting, {0}, offsetof(_STRUCT, _MEMBER), false, #_MEMBER, NULL, 0, _HF_PTR, NULL, NULL}
259
260/******************************************************************************
261 * M_NEXT_EXIST_LH(Par1, Par2, Par3)
262 * similar to the M_NEXT_EXIST except that instead of bit 0/1 which is fetched
263 * from the message in order to find out whether the next element/elements are
264 * present in the message, the logical operation XOR with the background
265 * pattern 0x2B is performed on the read bit before the decision is made.
266 *****************************************************************************/
267#define M_NEXT_EXIST_LH(_STRUCT, _MEMBER, _NoOfExisting, _HF_PTR)\
268 {CSN_NEXT_EXIST_LH, _NoOfExisting, {0}, offsetof(_STRUCT, _MEMBER), false, #_MEMBER, NULL, 0, _HF_PTR, NULL, NULL}
269
270/******************************************************************************
271 * M_NEXT_EXIST_OR_NULL(Par1, Par2, Par3)
272 * Similar to the M_NEXT_EXIST except that not only bit 0 or 1 but also the end
273 * of the message may be encountered when looking for the next element in the
274 * message.
275 * Covers the case {null | 0 | 1 < IE >}
276 *****************************************************************************/
277#define M_NEXT_EXIST_OR_NULL(_STRUCT, _MEMBER, _NoOfExisting, _HF_PTR)\
278 {CSN_NEXT_EXIST, _NoOfExisting, {0}, offsetof(_STRUCT, _MEMBER), true, #_MEMBER, NULL, 0, _HF_PTR, NULL, NULL}
279
280/******************************************************************************
281 * M_NEXT_EXIST_OR_NULL_LH(Par1, Par2, Par3)
282 * Similar to the M_NEXT_EXIST_LH except that not only bit 0 or 1 but also the
283 * end of the message may be encountered when looking for the next element in
284 * the message.
285 * Covers the case {null | L | H < IE >}
286 *****************************************************************************/
287#define M_NEXT_EXIST_OR_NULL_LH(_STRUCT, _MEMBER, _NoOfExisting, _HF_PTR)\
288 {CSN_NEXT_EXIST_LH, _NoOfExisting, {(void*)1}, offsetof(_STRUCT, _MEMBER), true, #_MEMBER, NULL, 0, _HF_PTR, NULL, NULL}
289
290/******************************************************************************
291 * M_UINT(Par1, Par2, Par3, Par4)
292 * Defines an integer number.
293 * Par1: C structure name
294 * Par2: C structure element name
295 * Par3: number of bits used to code the element (between 1 and 32)
296 * Par4: pointer to the header field
297 *****************************************************************************/
298#define M_UINT(_STRUCT, _MEMBER, _BITS, _HF_PTR)\
299 {CSN_UINT, _BITS, {0}, offsetof(_STRUCT, _MEMBER), false, #_MEMBER, NULL, 0, _HF_PTR, NULL, NULL}
300
301/******************************************************************************
302 * M_UINT_SPLIT(Par1, Par2, Par3, Par4)
303 * Defines an integer number split into segments which may be reordered or have gaps between them.
304 * Par1: C structure name
305 * Par2: C structure element name
306 * Par3: bits_spec_t array
307 * Par4: bit-width of the aggregate field
308 * Par4: pointer to the header field
309 *****************************************************************************/
310#define M_SPLIT_BITS(_STRUCT, _MEMBER, _SPEC, _BITS, _HF_PTR)\
311 {CSN_SPLIT_BITS, _BITS, {_SPEC}, offsetof(_STRUCT, _MEMBER), false, #_MEMBER, NULL, 0, _HF_PTR, NULL, NULL}
312
313/******************************************************************************
314 * M_NULL_SPLIT(Par1, Par2, Par3, Par4)
315 * Defines a subsequent segment of a split integer type.
316 * Par1: C structure name
317 * Par2: C structure element name
318 * Par3: bits_spec_t array
319 * Par4: segment number (0 based)
320 *****************************************************************************/
321#define M_BITS_CRUMB(_STRUCT, _MEMBER, _SPEC, _SEG, _HF_PTR)\
322 {CSN_SPLIT_BITS_CRUMB, _SEG, {_SPEC}, 0, false, #_MEMBER, NULL, 0, _HF_PTR, NULL, NULL}
323
324/******************************************************************************
325 * M_UINT_OR_NULL(Par1, Par2, Par3, Par4)
326 * Similar to the M_UINT except that not only the request set of bits but also the
327 * end of the message may be encountered when looking for the next element in
328 * the message.
329 * Covers the case {null | 0 | 1 < IE >}
330 *****************************************************************************/
331#define M_UINT_OR_NULL(_STRUCT, _MEMBER, _BITS, _HF_PTR)\
332 {CSN_UINT, _BITS, {0}, offsetof(_STRUCT, _MEMBER), true, #_MEMBER, NULL, 0, _HF_PTR, NULL, NULL}
333
334/******************************************************************************
335 * M_UINT_LH(Par1, Par2, Par3, Par4)
336 * This macro has the same functionality as M_UINT except that in addition the
337 * logical "exclusive or" operation with the background value "0x2B" is
338 * performed before the final value of the integer number is delivered from the
339 * received CSN.1 message
340 *****************************************************************************/
341#define M_UINT_LH(_STRUCT, _MEMBER, _BITS, _HF_PTR)\
342 {CSN_UINT_LH, _BITS, {0}, offsetof(_STRUCT, _MEMBER), false, #_MEMBER, NULL, 0, _HF_PTR, NULL, NULL}
343
344/******************************************************************************
345 * M_UINT_OFFSET(Par1, Par2, Par3, Par4)
346 * Defines an integer number.
347 * Par1: C structure name
348 * Par2: C structure element name
349 * Par3: number of bits used to code the element (between 1 and 32)
350 * Par4: value added to the returned integer (offset)
351 *****************************************************************************/
352#define M_UINT_OFFSET(_STRUCT, _MEMBER, _BITS, _OFFSET, _HF_PTR)\
353 {CSN_UINT_OFFSET, _BITS, {(void*)_OFFSET}, offsetof(_STRUCT, _MEMBER), false, #_MEMBER, NULL, 0, _HF_PTR, NULL, NULL}
354
355/******************************************************************************
356 * M_UINT_ARRAY(Par1, Par2, Par3, Par4)
357 * Defines an array of integer numbers. The size of the array is fixed.
358 * Par1: C structure name
359 * Par2: C structure element name
360 * Par3: number of bits used to code the each integer element (between 1 and 32)
361 * Par4: number of elements in the array (fixed integer value)
362 *****************************************************************************/
363#define M_UINT_ARRAY(_STRUCT, _MEMBER, _BITS, _ElementCount, _HF_PTR)\
364 {CSN_UINT_ARRAY, _BITS, {(void*)_ElementCount}, offsetof(_STRUCT, _MEMBER), false, #_MEMBER, NULL, 0, _HF_PTR, NULL, NULL}
365
366/******************************************************************************
367 * M_VAR_UINT_ARRAY(Par1, Par2, Par3, Par4)
368 * Defines an array of integer numbers. The size of the array is variable.
369 * Par1: C structure name
370 * Par2: C structure element name
371 * Par3: number of bits used to code the each integer element (between 1 and 32)
372 * Par4: number of elements in the array supplied by reference to the
373 * structure member holding the length value
374 *****************************************************************************/
375#define M_VAR_UINT_ARRAY(_STRUCT, _MEMBER, _BITS, _ElementCountField, _HF_PTR)\
376 {CSN_UINT_ARRAY, _BITS, {(void*)offsetof(_STRUCT, _ElementCountField)}, offsetof(_STRUCT, _MEMBER), false, #_MEMBER, NULL, 1, _HF_PTR, NULL, NULL}
377
378/******************************************************************************
379 * M_VAR_ARRAY(Par1, Par2, Par3, Par4)
380 * Defines an array of 8 bit large integer numbers. The size of the array is variable.
381 * Par1: C structure name
382 * Par2: C structure element name
383 * Par3: name of the structure member holding the size of the array
384 * Par4: offset that is added to the Par3 to get the actual size of the array
385 *****************************************************************************/
386#define M_VAR_ARRAY(_STRUCT, _MEMBER, _ElementCountField, _OFFSET, _HF_PTR)\
387 {CSN_VARIABLE_ARRAY, _OFFSET, {(void*)offsetof(_STRUCT, _ElementCountField)}, offsetof(_STRUCT, _MEMBER), false, #_MEMBER, NULL, 0, _HF_PTR, NULL, NULL}
388
389/******************************************************************************
390 * M_VAR_TARRAY(Par1, Par2, Par3, Par4)
391 * Similar to M_TYPE_ARRAY except that the size of the array is variable.
392 * Par1: C structure name
393 * Par2: C structure element name
394 * Par3: the type of each element of the array
395 * Par4: name of the structure member holding the size of the array
396 *****************************************************************************/
397#define M_VAR_TARRAY(_STRUCT, _MEMBER, _MEMBER_TYPE, _ElementCountField)\
398 {CSN_VARIABLE_TARRAY, offsetof(_STRUCT, _ElementCountField), {(const void*)CSNDESCR_##_MEMBER_TYPE}, offsetof(_STRUCT, _MEMBER), false, #_MEMBER, NULL, sizeof(_MEMBER_TYPE), NULL, NULL, NULL}
399
400/******************************************************************************
401 * M_VAR_TARRAY_OFFSET(Par1, Par2, Par3, Par4)
402 * Same as M_VAR_TARRAY with offset
403 *****************************************************************************/
404#define M_VAR_TARRAY_OFFSET(_STRUCT, _MEMBER, _MEMBER_TYPE, _ElementCountField)\
405 {CSN_VARIABLE_TARRAY_OFFSET, offsetof(_STRUCT, _ElementCountField), {(const void*)CSNDESCR_##_MEMBER_TYPE}, offsetof(_STRUCT, _MEMBER), false, #_MEMBER, NULL, sizeof(_MEMBER_TYPE), NULL, NULL, NULL}
406
407/******************************************************************************
408 * M_REC_ARRAY(Par1, Par2, Par3, Par4)
409 * similar to the M_VAR_ARRAY. The difference is that the size of the array is
410 * not known in advance and it has to be calculated during unpacking. Its value
411 * is stored in a variable which belongs to the same structure as the array.
412 * A zero element terminates the array. The CSN.1 syntax describes it
413 * recursively as:
414 * <array> ::={1 <element> <array>| 0}
415 *
416 * Par1: C structure name
417 * Par2: C structure element name
418 * Par3: name of the structure member where the calculated the size of the
419 * array will be stored
420 * Par4: length of each element in bits
421 *****************************************************************************/
422/* XXX - need 2 hf support */
423#define M_REC_ARRAY(_STRUCT, _MEMBER, _ElementCountField, _BITS, _HF_PTR, _HF_PTR_EXIST)\
424 {CSN_RECURSIVE_ARRAY, _BITS, {(const void*)offsetof(_STRUCT, _ElementCountField)}, offsetof(_STRUCT, _MEMBER), false, #_MEMBER, NULL, 0, _HF_PTR, _HF_PTR_EXIST, NULL}
425
426/******************************************************************************
427 * M_VAR_TYPE_ARRAY(Par1, Par2, Par3, Par4)
428 * Defines an array of structures. The size of the array is variable.
429 * Par1: C structure name
430 * Par2: C structure element name
431 * Par3: name of the structure
432 * Par4: number of elements in the array (fixed integer value)
433 *****************************************************************************/
434#define M_TYPE_ARRAY(_STRUCT, _MEMBER, _MEMBER_TYPE, _ElementCount)\
435 {CSN_TYPE_ARRAY, _ElementCount, {(const void*)CSNDESCR_##_MEMBER_TYPE}, offsetof(_STRUCT, _MEMBER), false, #_MEMBER, NULL, sizeof(_MEMBER_TYPE), NULL, NULL, NULL}
436
437/******************************************************************************
438 * M_REC_TARRAY(Par1, Par2, Par3, Par4)
439 * Defines an recursive array of structures. The size of the array is variable.
440 * <list> ::= {1 <type>} ** 0 ;
441 * Par1: C structure name
442 * Par2: C structure element name
443 * Par3: name of the structure
444 * Par4: will hold the number of element in the array after unpacking
445 *****************************************************************************/
446#define M_REC_TARRAY(_STRUCT, _MEMBER, _MEMBER_TYPE, _ElementCountField, _HF_PTR)\
447 {CSN_RECURSIVE_TARRAY, offsetof(_STRUCT, _ElementCountField), {(const void*)CSNDESCR_##_MEMBER_TYPE}, offsetof(_STRUCT, _MEMBER), false, #_MEMBER, NULL, sizeof(_MEMBER_TYPE), _HF_PTR, NULL, (void_fn_t)array_length(((_STRUCT*)0)->_MEMBER)}
448
449/******************************************************************************
450 * M_REC_TARRAY1(Par1, Par2, Par3, Par4)
451 * Same as M_REC_TARRAY but first element always exist:
452 * <list> ::= <type> {1 <type>} ** 0 ;
453 *****************************************************************************/
454#define M_REC_TARRAY_1(_STRUCT, _MEMBER, _MEMBER_TYPE, _ElementCountField, _HF_PTR)\
455 {CSN_RECURSIVE_TARRAY_1, offsetof(_STRUCT, _ElementCountField), {(const void*)CSNDESCR_##_MEMBER_TYPE}, offsetof(_STRUCT, _MEMBER), false, #_MEMBER, NULL, sizeof(_MEMBER_TYPE), _HF_PTR, NULL, (void_fn_t)array_length(((_STRUCT*)0)->_MEMBER)}
456
457/******************************************************************************
458 * M_REC_TARRAY2(Par1, Par2, Par3, Par4)
459 * Same as M_REC_TARRAY but with reversed separators :
460 * <lists> ::= <type> { 0 <type> } ** 1 ;
461 *****************************************************************************/
462#define M_REC_TARRAY_2(_STRUCT, _MEMBER, _MEMBER_TYPE, _ElementCountField)\
463 {CSN_RECURSIVE_TARRAY_2, offsetof(_STRUCT, _ElementCountField), {(const void*)CSNDESCR_##_MEMBER_TYPE}, offsetof(_STRUCT, _MEMBER), false, #_MEMBER, NULL, sizeof(_MEMBER_TYPE), NULL, NULL, (void_fn_t)array_length(((_STRUCT*)0)->_MEMBER)}
464
465/******************************************************************************
466 * M_TYPE(Par1, Par2, Par3)
467 * Defines a reference to a structure which is described elsewhere
468 * <list> ::= {1 <type>} ** 0 ;
469 * Par1: C structure name
470 * Par2: C structure element name
471 * Par3: type of member
472 *****************************************************************************/
473#define M_TYPE(_STRUCT, _MEMBER, _MEMBER_TYPE)\
474 {CSN_TYPE, 0, {(const void*)CSNDESCR_##_MEMBER_TYPE}, offsetof(_STRUCT, _MEMBER), false, #_MEMBER, NULL, 0, NULL, NULL, NULL}
475
476/******************************************************************************
477 * M_TYPE_OR_NULL(Par1, Par2, Par3)
478 * Similar to the M_TYPE except that not only the request set of bits but also the
479 * end of the message may be encountered when looking for the next element in
480 * the message.
481 * Covers the case {null | 0 | 1 < IE >}
482 *****************************************************************************/
483#define M_TYPE_OR_NULL(_STRUCT, _MEMBER, _MEMBER_TYPE)\
484 {CSN_TYPE, 0, {(const void*)CSNDESCR_##_MEMBER_TYPE}, offsetof(_STRUCT, _MEMBER), true, #_MEMBER, NULL, 0, NULL, NULL, NULL}
485
486
487/******************************************************************************
488 * M_TYPE_LABEL(Par1, Par2, Par3, Par4)
489 * Same as M_TYPE but allows to define a custom string for the subtree
490 * <list> ::= {1 <type>} ** 0 ;
491 * Par1: C structure name
492 * Par2: C structure element name
493 * Par3: type of member
494 * Par4: C string for the text
495 *****************************************************************************/
496#define M_TYPE_LABEL(_STRUCT, _MEMBER, _MEMBER_TYPE, _LABEL)\
497 {CSN_TYPE, 0, {(const void*)CSNDESCR_##_MEMBER_TYPE}, offsetof(_STRUCT, _MEMBER), false, _LABEL, NULL, 0, NULL, NULL, NULL}
498
499/******************************************************************************
500 * M_UNION(Par1, Par2)
501 * Informs the CSN.1 library that a union follows and how many possible choices
502 * there are in the union. The actual value of the choice, which points out the
503 * chosen element of the union is stored in the uint8 variable and is usually
504 * called UnionType. The elements of the union have to be listed directly after
505 * the M_UNION statement.
506 * Par1: C structure name
507 * Par2: number of possible choice in the union
508 *****************************************************************************/
509#define M_UNION(_STRUCT, _COUNT, _HF_PTR)\
510 {CSN_UNION, _COUNT, {0}, offsetof(_STRUCT, UnionType), false, "UnionType", NULL, 0, _HF_PTR, NULL, NULL}
511
512/******************************************************************************
513 * M_UNION_LH(Par1, Par2)
514 * Same as M_UNION but masked with background value 0x2B
515 *****************************************************************************/
516#define M_UNION_LH(_STRUCT, _COUNT, _HF_PTR)\
517 {CSN_UNION_LH, _COUNT, {0}, offsetof(_STRUCT, UnionType), false, "UnionType", NULL, 0, _HF_PTR, NULL, NULL}
518
519/******************************************************************************
520 * M_CHOICE(Par1, Par2, Par3, Par4)
521 * Similar to the M_UNION. In the M_UNION the selected element of all possible
522 * choices in the union is referred as a sequential numbers, i.e., the first
523 * choice is addressed as choice 0 the second as choice 1, the third as choice
524 * 2 and so on, both in the encoded message and in the variable UnionType which
525 * is the part of the message. In the CSN_CHOICE case, this rule does not
526 * apply. There is free but predefined mapping of the element of the union and
527 * the value which addresses this element.
528 * The value of the address is called a selector.
529 * After unpacking, this value is then converted to the sequential number of the
530 * element in the union and stored in the UnionType variable.
531 * Par1: C structure name
532 * Par2: C structure element name
533 * Par3: address of an array of type CSN_ChoiceElement_t where all possible
534 * values of the selector are provided, together with the selector
535 * length expressed in bits and the address of the CSN_DESCR type
536 * where the element is defined. For every element in the union
537 * there is one line in the Choice variable. These lines have to
538 * appear in the _CHOICE in the same order as the elements in the
539 * union. The element of the union selected in the message through
540 * the _CHOICE parameter is after unpacking translated to the
541 * corresponding sequential number of this element and stored in
542 * the variable pointed out by the _MEMBER
543 * Par4: number of possible choices in the union
544 *****************************************************************************/
545#define M_CHOICE(_STRUCT, _MEMBER, _CHOICE, _ElementCount, _HF_PTR)\
546 {CSN_CHOICE, _ElementCount, {(const void*)_CHOICE}, offsetof(_STRUCT, _MEMBER), false, #_CHOICE, NULL, 0, _HF_PTR, NULL, NULL}
547
548/******************************************************************************
549 * M_CHOICE_IL(Par1, Par2, Par3, Par4)
550 * See M_CHOICE above, but displayed inline (i.e. no specific elements are
551 * displayed to show there was a choice
552 *****************************************************************************/
553#define M_CHOICE_IL(_STRUCT, _MEMBER, _CHOICE, _ElementCount, _HF_PTR)\
554 {CSN_CHOICE, _ElementCount, {(const void*)_CHOICE}, offsetof(_STRUCT, _MEMBER), false, NULL, NULL, 0, _HF_PTR, NULL, NULL}
555
556/******************************************************************************
557 * M_FIXED(Par1, Par2, Par3)
558 * Defines a fixed value of type integer which should be fetched from or stored
559 * in the message
560 * Par1: C structure name
561 * Par2: gives the length of the fixed number in bits.
562 * Par3: the value of the number. If the expected value is not present in
563 * the message the unpacking procedure is aborted
564 *****************************************************************************/
565#define M_FIXED(_STRUCT, _BITS, _BITVALUE, _HF_PTR)\
566 {CSN_FIXED, _BITS, {0}, _BITVALUE, false, #_BITVALUE, NULL, 0, _HF_PTR, NULL, NULL}
567
568/******************************************************************************
569 * M_FIXED_LABEL(Par1, Par2, Par3, Par4)
570 * Same as M_FIXED but allows to define a custom string for the subtree
571 * Par1: C structure name
572 * Par2: gives the length of the fixed number in bits.
573 * Par3: the value of the number. If the expected value is not present in
574 * the message the unpacking procedure is aborted
575 * Par4: C string for the text
576 *****************************************************************************/
577#define M_FIXED_LABEL(_STRUCT, _BITS, _BITVALUE, _LABEL, _HF_PTR)\
578 {CSN_FIXED, _BITS, {0}, _BITVALUE, false, _LABEL, NULL, 0, _HF_PTR, NULL, NULL}
579
580/******************************************************************************
581 * M_SERIALIZE(Par1, Par2, Par3)
582 * Allows using a complete free format of data being encoded or decoded.
583 * When the M_SERIALIZE is encounted during encoding or decoding of a message
584 * the CSNstream program passes the control over to the specified function
585 * together with all necessary parameters about the current position within
586 * the message being unpacked or packed. When transferring of "serialized"
587 * data to or from the message is finished by the function the CSNstream gets
588 * back control over the data stream and continues to work with the message.
589 *****************************************************************************/
590#define M_SERIALIZE(_STRUCT, _MEMBER, _LENGTH_LEN, _HF_PTR, _SERIALIZEFCN)\
591 {CSN_SERIALIZE, _LENGTH_LEN, {0}, offsetof(_STRUCT, _MEMBER), false, #_MEMBER, NULL, 0, _HF_PTR, NULL, (void_fn_t)_SERIALIZEFCN}
592
593#define M_CALLBACK(_STRUCT, _CSNCALLBACKFCN, _PARAM1, _PARAM2)\
594 {CSN_CALLBACK, offsetof(_STRUCT, _PARAM1), {0}, offsetof(_STRUCT, _PARAM2), false, "CallBack_"#_CSNCALLBACKFCN, NULL, 0, NULL, NULL, (void_fn_t)_CSNCALLBACKFCN}
595
596/******************************************************************************
597 * M_BITMAP(Par1, Par2, Par3)
598 * Defines a type which consists of a bitmap. The size of the bitmap in bits
599 * is fixed and provided by the parameter Par3
600 * Par1: C structure name
601 * Par2: C structure element name
602 * Par3: length of the bitmap expressed in bits
603 *****************************************************************************/
604#define M_BITMAP(_STRUCT, _MEMBER, _BITS, _HF_PTR)\
605 {CSN_BITMAP, _BITS, {0}, offsetof(_STRUCT, _MEMBER), false, #_MEMBER, NULL, 0, _HF_PTR, NULL, NULL}
606
607/* variable length, right aligned bitmap i.e. _ElementCountField = 11 => 00000111 11111111 */
608#define M_VAR_BITMAP(_STRUCT, _MEMBER, _ElementCountField, _OFFSET, _HF_PTR)\
609 {CSN_VARIABLE_BITMAP, _OFFSET, {(void*)offsetof(_STRUCT, _ElementCountField)}, offsetof(_STRUCT, _MEMBER), false, #_MEMBER, NULL, 0, _HF_PTR, NULL, NULL}
610
611/* variable length, right aligned bitmap filling the rest of message
612 * - when unpacking the _ElementCountField will be set in runtime
613 * - when packing _ElementCountField contains the size of bitmap
614 */
615#define M_VAR_BITMAP_1(_STRUCT, _MEMBER, _ElementCountField, _OFFSET)\
616 {CSN_VARIABLE_BITMAP_1, _OFFSET, {(void*)offsetof(_STRUCT, _ElementCountField)}, offsetof(_STRUCT, _MEMBER), false, #_MEMBER, NULL, 0, NULL, NULL, NULL}
617
618/* variable length, left aligned bitmap i.e. _ElementCountField = 11 => 11111111 11100000 */
619#define M_LEFT_VAR_BMP(_STRUCT, _MEMBER, _ElementCountField, _OFFSET, _HF_PTR)\
620 {CSN_LEFT_ALIGNED_VAR_BMP, _OFFSET, {(void*)offsetof(_STRUCT, _ElementCountField)}, offsetof(_STRUCT, _MEMBER), false, #_MEMBER, NULL, 0, _HF_PTR, NULL, NULL}
621
622/* variable length, left aligned bitmap filling the rest of message
623 *- when unpacking the _ElementCountField will be set in runtime
624 * - when packing _ElementCountField contains the size of bitmap
625 */
626#define M_LEFT_VAR_BMP_1(_STRUCT, _MEMBER, _ElementCountField, _OFFSET, _HF_PTR)\
627 {CSN_LEFT_ALIGNED_VAR_BMP_1, _OFFSET, {(void*)offsetof(_STRUCT, _ElementCountField)}, offsetof(_STRUCT, _MEMBER), false, #_MEMBER, NULL, 0, _HF_PTR, NULL, NULL}
628
629/* todo: dissect padding bits looking for unexpected extensions */
630#define M_PADDING_BITS(_STRUCT, _HF_PTR)\
631 {CSN_PADDING_BITS, 0, {0}, 0, true, "Padding", NULL, 0, _HF_PTR, NULL, NULL}
632
633#define M_NULL(_STRUCT, _MEMBER, _SKIP_BITS)\
634 {CSN_NULL, _SKIP_BITS, {0}, offsetof(_STRUCT, _MEMBER), false, #_MEMBER, NULL, 0, NULL, NULL, NULL}
635
636#define M_THIS_EXIST(_STRUCT, _HF_PTR)\
637 {CSN_EXIST, 0, {0}, offsetof(_STRUCT, Exist), false, "Exist", NULL, 0, _HF_PTR, NULL, NULL}
638
639#define M_THIS_EXIST_LH(_STRUCT, _HF_PTR)\
640 {CSN_EXIST_LH, 0, {0}, offsetof(_STRUCT, Exist), false, "Exist", NULL, 0, _HF_PTR, NULL, NULL}
641
642/* return value 0 if ok else discontinue the unpacking */
643typedef int16_t (*CsnCallBackFcn_t)(void* pv ,...);
644
645#define CSNDESCR(_FuncType) CSNDESCR_##_FuncType
646
647#endif /*_PACKET_CSN1_H_*/
648
649/*
650 * Editor modelines - https://www.wireshark.org/tools/modelines.html
651 *
652 * Local Variables:
653 * c-basic-offset: 2
654 * tab-width: 8
655 * indent-tabs-mode: nil
656 * End:
657 *
658 * vi: set shiftwidth=2 tabstop=8 expandtab:
659 * :indentSize=2:tabSize=8:noTabs=true:
660 */
array.h
expert.h
_packet_info
Definition packet_info.h:43
_proto_node
Definition proto.h:907
CSN_ChoiceElement_t
Definition packet-csn1.h:184
CSN_DESCR
Definition packet-csn1.h:162
crumb_spec_t
Definition proto.h:841
csnStream_t
Definition packet-csn1.h:48
expert_field
Definition expert.h:39
tvbuff
Definition tvbuff-int.h:35