| Wireshark 4.7.0 The Wireshark network protocol analyzer

Loading...
Searching...
No Matches
packet-6lowpan.h
1/* packet-6lowpan.h
2 * Routines for 6LoWPAN packet disassembly
3 *
4 * SPDX-License-Identifier: GPL-2.0-or-later
5 */
6
7#ifndef __PACKET_6LOWPAN_H__
8#define __PACKET_6LOWPAN_H__
9
10#include <wsutil/inet_addr.h>
11
12/* Inserts new compression context information into the 6LoWPAN context table.
13 * The compression context is distributed via some options added to the neighbor
14 * discovery protocol, so the ICMPv6 dissector needs to call this routine.
15 */
16extern void lowpan_context_insert(uint8_t cid, uint16_t pan, uint8_t plen,
17 ws_in6_addr *prefix, unsigned frame);
18
19#endif /* __PACKET_6LOWPAN_H__ */
inet_addr.h
e_in6_addr
Represents a 128-bit IPv6 address.
Definition inet_addr.h:27