| Wireshark 4.7.0 The Wireshark network protocol analyzer

Loading...
Searching...
No Matches
Macros | Variables
afn.h File Reference

Go to the source code of this file.

## Macros
#define | AFNUM_RESERVED 0 /* Reserved */
#define | AFNUM_INET 1 /* IP (IP version 4) */
#define | AFNUM_INET6 2 /* IP6 (IP version 6) */
#define | AFNUM_NSAP 3 /* NSAP */
#define | AFNUM_HDLC 4 /* HDLC (8-bit multidrop) */
#define | AFNUM_BBN1822 5 /* BBN 1822 */
#define | AFNUM_802 6 /* 802 (includes all 802 media plus Ethernet "canonical format") */
#define | AFNUM_E163 7 /* E.163 */
#define | AFNUM_E164 8 /* E.164 (SMDS, Frame Relay, ATM) */
#define | AFNUM_F69 9 /* F.69 (Telex) */
#define | AFNUM_X121 10 /* X.121 (X.25, Frame Relay) */
#define | AFNUM_IPX 11 /* IPX */
#define | AFNUM_ATALK 12 /* Appletalk */
#define | AFNUM_DECNET 13 /* Decnet IV */
#define | AFNUM_BANYAN 14 /* Banyan Vines */
#define | AFNUM_E164NSAP 15 /* E.164 with NSAP format subaddress */
#define | AFNUM_DNS 16 /* DNS (Domain Name System) */
#define | AFNUM_DISTNAME 17 /* Distinguished Name */
#define | AFNUM_AS_NUMBER 18 /* AS Number */
#define | AFNUM_XTP_IP4 19 /* XTP over IP version 4 */
#define | AFNUM_XTP_IP6 20 /* XTP over IP version 6 */
#define | AFNUM_XTP 21 /* XTP native mode XTP */
#define | AFNUM_FC_WWPN 22 /* Fibre Channel World-Wide Port Name */
#define | AFNUM_FC_WWNN 23 /* Fibre Channel World-Wide Node Name */
#define | AFNUM_GWID 24 /* GWID */
#define | AFNUM_L2VPN 25 /* RFC4761 RFC6074 */
#define | AFNUM_L2VPN_OLD 196
#define | AFNUM_MPLS_TP_SEI 26 /* MPLS-TP Section Endpoint Identifier, RFC7212 */
#define | AFNUM_MPLS_TP_LSPEI 27 /* MPLS-TP LSP Endpoint Identifier, RFC7212 */
#define | AFNUM_MPLS_TP_PEI 28 /* MPLS-TP Pseudowire Endpoint Identifier, RFC7212 */
#define | AFNUM_MT_IP 29 /* MT IP: Multi-Topology IP version 4, RFC7307 */
#define | AFNUM_MT_IPV6 30 /* MT IPv6: Multi-Topology IP version 6, RFC7307 */
#define | AFNUM_EIGRP_COMMON 16384 /* EIGRP Common Service Family, Donnie Savage */
#define | AFNUM_EIGRP_IPV4 16385 /* EIGRP IPv4 Service Family, Donnie Savage */
#define | AFNUM_EIGRP_IPV6 16386 /* EIGRP IPv6 Service Family, Donnie Savage */
#define | AFNUM_LCAF 16387 /* LISP Canonical Address Format, David Meyer */
#define | AFNUM_BGP_LS 16388 /* BGP-LS, RFC7752 */
#define | AFNUM_EUI48 16389 /* 48-bit MAC, RFC7042 */
#define | AFNUM_EUI64 16390 /* 64-bit MAC, RFC7042 */
#define | AFNUM_OUI 16391 /* OUI, RFC7961 */
#define | AFNUM_MAC_24 16392 /* MAC/24, RFC7961 */
#define | AFNUM_MAC_40 16393 /* MAC/40, RFC7961 */
#define | AFNUM_IPv6_64 16394 /* IPv6/64, RFC7961 */
#define | AFNUM_RB_PID 16395 /* RBridge Port ID, RFC7961 */
#define | AFNUM_TRILL_NICKNAME 16396 /* TRILL Nickname, RFC7455 */

## Variables
const value_string | afn_vals []

## Detailed Description

RFC 1700 address family numbers

Wireshark - Network traffic analyzer By Gerald Combs geral.nosp@m.d@wi.nosp@m.resha.nosp@m.rk.o.nosp@m.rg Copyright 1998 Gerald Combs

SPDX-License-Identifier: GPL-2.0-or-later